|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sr. #** | **Name** | **Usage** | **Specification** | **Remarks** |
| 1 | MQ-2 | Methane, Butane, LPG, **smoke** | Detection range: 300 -10000 ppm  Operating Voltage: +5V  Output: Analog | Used |
| 2 | MQ-7 | **Carbon Monoxide** | Detection range: 20 - 2000ppm  Operating Voltage: +5V  Output: Analog | Used |
| 3 | MQ-9 | Carbon Monoxide, **Methane, Propane** | Detection range: 20 - 10000 ppm  Operating Voltage: +5V  Output: Analog | Used |
| 4 | MQ-135 | **Air Quality** (CO, NH3, NO2, Alcohol, CO2) | Detection range: 300-2000 ppm  Operating Voltage: +5V  Output: Analog | Used |
| 5 | DS18b20 | Temperature sensor | --- | Not Used |
| 6 | HR202 | Humidity Sensor Module | --- | Not Used |
| 7 |  |  |  |  |